{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Main","Лист3"],"not_rendered":{"charts":0,"images":13,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Main","index":0,"n_rows":90,"n_cols":9,"rows_kept":90,"cut":false,"hidden":false,"merged":[[8,2,8,3],[1,2,1,3],[3,2,3,3],[7,2,7,3],[0,7,0,8],[0,4,0,5]]}
["указатель",null,null,null,"Пакетные команды",null,null,"список команд"]
["ком порт",null,"Читать ключи",null,null,null,null,"символ","описание"]
[null,null,"        Читать","Прекратить    ",null,"Количество повторов",null,"A","Выдать  12В на  контакт POWER"]
["Конвертер","Отключен","Конвертировать",null,null,5,null,"Z","Отключить  12В на  контакте POWER"]
[null,null,null,null,null,null,null,"X","Выдать  5В на  контакт BEEP"]
["подключить",null,null,null,null,"Мастер ключ",null,"S","Выдать  0В на  контакт BEEP"]
[null,null,null,null,null,null,null,"V","Выдать  5В на  контакт LED G"]
[null,null,"Передать ключи",null,"название ","строка пакета",null,"F","Выдать  0В на  контакт LED G"]
["отключить",null,null,null,"Добавление ключей","T600K100N",null,"C","Выдать  5В на  контакт LED R"]
[null,null,"Текущий","off","передаем все ключи","G100N",null,"D","Выдать  0В на  контакт LED R"]
[null,null,null,null,"передать мастер ключ","T50K",null,"T","Начать передачу мастер ключа"]
["описание",null,"Все",null,null,null,null,"K","Остановить передачу мастер ключа "]
[null,null,null,null,"Удаление ключей","T50K200T50K200T600K100N",null,"Y","Передать карты отмеченные Y"]
[null,null,"Отмеченные",null,"отмеченные W","W50N",null,"W","Передать карты отмеченные W"]
["Записать номер мастер",null,null,null,"передать мастер ключ","T50K",null,"G","Передать все карты"]
["ключа для пакетной",null,"контакт",30,null,null,null,"N","Переход на следующую строку пакета"]
[" команды в ячейку F7",null,"пауза",30,"Добавление ключей","T600K100N",null,"P","Повторить строку команды"]
["(не в контроллер)",null,null,null,"отмеченные W","W50N",null,"M","Добавить мастер ключ(и)"]
["тип","номер","ключи из BaseZ5R","флаг","передать мастер ключ","T50K"]
[]
[null,null,null,null,"стираем всю память","T50K200T50K200T50K200T600K100"]
[]
[null,null,null,null,"время открывания замка","T50K200T50K200T50K200T50K200N"]
[null,null,null,null,"0 на \"кнопка\"","S300X"]
[null,null,null,null,null,"W"]
[null,null,null,null,null,"Y"]
[]
[null,null,null,null,null,"S50X"]
[]
[null,null,null,null,"Подать питание","A"]
[null,null,null,null,"Снять питание","Z"]
[null,null,null,null,"передать мастер ключ","T50K"]
[]
[null,null,null,null,"звук","S50X50P"]
[null,null,null,null,"Led G","F50V50P"]
[null,null,null,null,"Led R","D50C50P"]
[]
[]
[null,null,null,null,"отключаем питание","A300DDDN"]
[null,null,null,null,"+5 на \"кнопка\"","Z80VVVN"]
[null,null,null,null,"включаем питание","A300N"]
[null,null,null,null,"время открывания замка","Z80DDDDDDDDDDN"]
[null,null,null,null,"0 на \"кнопка\" - 0,3 сек.","A300"]
[]
[]
[null,null,null,null,"Удаление ключей","T50K200T50K200T600K200"]
[null,null,null,null,null,"T30K150N"]
[null,null,null,null,null,"T600K200N"]
[null,null,null,null,"отмеченные Y","Y100N"]
[null,null,null,null,"передать мастер ключ","T50K"]
[]
[null,null,null,null,"Добавить мастер ключ(и)","T50K200T600K100N"]
[null,null,null,null,"отмеченные M","M50N"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"      "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"                              "]

{"sheet":"Лист3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}